;Watts Per Square Foot##ELECTRICAL_WATTAGE##WATTS;Power##OTHER##;Width##LENGTH##INCHES;Height##LENGTH##INCHES;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Type Check##OTHER##
400 - One Round-Style Junction Box - 120-277V;400;120 V, 208 - 277 V and 1 or 3 phase;36;24;277;0
400 - One Round-Style Junction Box - 120-480V;400;120 V, 208 - 277 V, 480 V and 1 or 3 phase;108;80;480;1
400 - Two Round-Style Junction Boxes - 120-480V;400;120 V, 208 - 277 V, 480 V and 3 phase;160;99;480;2
400 - One Rectangular Junction Box - 120-277V;400;120 V, 208 - 277 V and 1 or 3 phase;36;24;277;3
400 - One Rectangular Junction Box - 120-480V;400;120 V, 208 - 277 V, 480 V and 1 or 3 phase;108;80;480;4
400 - Two Rectangular Junction Boxes - 120-480V;400;120 V, 208 - 277 V, 480 V and 3 phase;160;99;480;5
800 - One Rectangular Junction Box - 208-480V;800;208 - 277 V, 480 V and 1 or 3 phase;108;80;480;6
800 - Two Rectangular Junction Boxes - 208-480V;800;208 - 277 V, 480 V and 3 phase;160;99;480;7
1600 - One Rectangular Junction Box - 208-480V;1600;208 - 277 V, 480 V and 1 or 3 phase;108;80;480;8
1600 - Two Rectangular Junction Boxes - 208-480V;1600;208 - 277 V, 480 V and 3 phase;160;99;480;9
